README.TXT For REALmagic Hollywood Plus drivers for Win 2000 
Release 2.0  (Build 129) ------ 8/25/00
=======================================
This file contains important information for the installation of 
the drivers and application software for the Hollywood Plus.

	      _____________________________________
			
	   FOR FUTURE updates DRIVERS VISIT OUR WEB SITE
		     www.sigmadesigns.com
              Latest Drivers & FTP Access - Hollywood Plus
		     ____________________

SOFTWARE RELEASE NOTICE
=======================

1 - If you are installing the Hollywood Plus for the first time, you
    need to set its region code by running SETUP from the application
    diskette.  If the DVD-ROM drive is an RPC2 drive - carrying its
    own region code - then you do not need to set a region code for
    Hollywood Plus.  Make sure you set a region code for the new 
    DVD-ROM drive - this can be achieved with the Windows utility in
    Device Manager\CD-ROM tab.   If you insert a movie with a region
    code mismatching the DVD-ROM drive region - for RPC2 drives, the
    tray will be ejected and a Windows error message issued. 
2 - The numeric keypad is not supported for the playback of SVCDs.
    You'll get the message "Invalid MCI device ID".
3 - The "Eject" button of the DVD Station needs to be pressed twice
    with DVD-ROM movies in the playback mode and only once in the 
    Stop mode.
4 - The installation will set DVD Station as the default player when
    you insert a DVD-ROM movie disc.
5 - For a clean Uninstall, please check section I.
6 - DTS audio is supported : whenever you choose the DTS option in a
    movie menu the OUTPUT WILL BE DIRECTED THRU THE SP/DIF OUPUT IN
    DIGITAL FORMAT REGARDLESS OF THE DVD STATION AUDIO OUPUT SETTING,
    so the DTS stream is NOT decoded thru the analog mini audio jack.
7 - The REALmagic logo is shifted in the opening screen of DVD Station.
8 - You need to be logging in as an Administrator or equivalent to
    install and use the Hollywood Plus.
9 - You can use the Hollywood Plus without the pass-thru cable, but
    in this case the video playback will be available on TV only
    (and not on the VGA monitor).  The system will detect the 
    presence of this cable at booting time.  So connecting or
    disconnecting it during a Windows session is not correct.
    A reboot is needed to notify the Hollywood Plus driver.
10- Some systems will exhibit a slight lip synch issue with some movies
    between video and audio on the external AC-3 decoder thru the S/PDIF.
    This will be fixed in next release.




CONTENTS
========					
I   - DRIVER AND APPLICATIONS INSTALLATION	
II  - BORDER ADJUSTMENT AND COLOR CALIBRATION	       
III - DVD REGION CODE CHANGE				
IV  - TV OUT
V   - FULL SCREEN PLAYBACK
VI  - HINTS TO RESOLVE PROBLEMS AND BETTER PLAYBACK



I   - DRIVER AND APPLICATIONS INSTALLATION
      ====================================
  
Note : You need to have the Administrator rights to be able to
       install this software because of its modifications to the
       registry.

1.  On booting your system, Windows 2K will detect the card. Insert the
    REALmagic Hollywood Plus Drivers Disk in your floppy drive A and 
    click Finish. This will install Hollywood Plus drivers on your hard
    disk.
2.  To install the DVD navigation software insert Application Disk into
    drive A and run SETUP.
3.  The Setup program will show two options: Install the REALmagic DVD
    application or Change the DVD region code.
4.  Check the DVD application installation option and follow the 
    instructions.  
5.  After the files are copied, set a DVD region code as part of the 
    setup program  (if not already set up under Win 9x or Win NT 4.0).
    Note: Setup will not ask you to set the DVD region code if this
    code is set in a previous installation.
6.  Click Finish to complete the installation process by performing
    Auto Calibration.  PLEASE REBOOT THE SYSTEM.

    Forcing a clean Uninstall :
    -------------------------
 a - delete the following files from \WINNT\SYSTEM32 and 
     \WINNT\SYSTEM32\DRIVERS :
        24 bits.dib, 4bits.dib, 8bits.dib, cross.vbs
     DLLs: AC3DLL, IMPEG32, MCIFMP32, MPEGAPI, SDUDF, WAVIFACE
     SYSs : MPEGPORT, RMDVD, RMQUASAR, VPFILTER, IMPEG32.EXE
 b - right-click "My Computer", select Hardware - Device Manager - 
     "Sound, Video,...." - double-click "Sigma Designs Hollywood Plus"-
     select Driver - click Uninstall.  This will uninstall the P-n-P.
 c - delete the same sub-entries in the Registry entry :
      HKEY_LOCAL_MACHINE - SYSTEM - CurrentControlSet - Services
 d - delete the OEMx.INF file from WINDOWS\INF (where x is a number
     depending on your system but the selected file should have the 
     "Sigma Designs ..." signature in its last two lines).



   
II - BORDER ADJUSTMENT AND COLOR CALIBRATION
     =======================================

    NOTE: If the border is not adjusted properly after Auto Calibration
          you may need to set the Border Adjustment to get more 
          accurate adjustment. You need to set the Border Adjustment 
          only once for each setting of display resolution.

1.  At the Start button, click Programs and select REALmagic Hollywood
    Plus program group. Click REALmagic Configuration.
2.  Click on Adjust Border and use the proper buttons to adjust the 
    black rectangle in the magenta box.
3.  Change different values to adjust stability if you are viewing 
    jumping pixels on MPEG video. Click OK when you are done. 
4.  The Reset Default button will reset the color calibration and 
    border adjustment values to the factory default settings.

    Note 1: Color calibration is required if the colors are not 
            normal or the screen is pink or not clear. If color 
            calibration is required, Click on "Auto Calibration". The
            screen will flash for 5 to 10 seconds then displays a 
            message that the calibration is complete. Click OK.
    Note 2: In the cases where this calibration is unsuccessful, 
            you can click on Advanced..., then the Manual 
            Calibration. This will involve fixing the R, G, B 
            sliders as shown in the window four times. You can use the
            up/down arrow keys for fine tuning and you don't need
            necessarily to see the cross but just the disappearance
            of the vertical bar.

III - DVD REGION CODE CHANGE
      ======================

1.  Run the set program from Application disk. Select DVD Region Code 
    change option. Set the region code according to the country you 
    are in.  You do NOT need to set the region code when Uninstalling/
    installing new drivers.
      _._._._._._._._._._._._._._._._._._._._._._._._._._._._._._._._
    Note: The setup program will allow you to change the region code 
          for five times. If you want to reset the region code settings
          after five times contact the card manufacturer or an 
          authorized distributor or service center. A nominal handling
          fee will be charged.

IV  - TV OUT
      ======

    The REALmagic Hollywood Plus can display on a VGA monitor or a TV.
    To switch between these modes an icon is provided on the left 
    corner of the DVD Station control panel that toggles between 
    computer monitor and TV.

    In order to display on a TV, some additional settings may be 
    required. From the DVD Station control panel click Options button.
    This will open a window for options setting. Click the settings tab.
    Select the options according to your TV type. The color control, 
    brightness, and contrast controls have also been provided for TV.

    Note :  Some TVs are sensitive with video frequency input and may 
            show Black and White video on TV. This has specially been
            noticed on some PAL TVs. In such a situation do the 
            following WHILE the TV-Out option is active and DVD/MPEG is
            playing on TV.:
		1. From the DVD station click the "Options Dialog -
                   Settings tab.
		2. Press Configure and then press Advanced Settings.
		3. Select Expert Settings and click the mouse. This 
                   will open a pop-up window. Adjust different values
                   until you have color picture on TV.  Notice that you
                   need to keep on going in one direction when changing
                   the values i.e. either always increasing or 
                   decreasing because of the hysteresis nature of this
                   adjustment.
     Some PAL TVs with SCART/S-Video adapters will not show 
     colors thru their S-Video inputs but will show a B&W picture.
     Either the TV set is not tuned to the proper channel or the
     TV set does not support S-Video input.
		     					

V  - FULL SCREEN PLAYBACK
     ====================

    In order to playback in full screen, double click the left button
    of mouse anywhere in the MPEG window or press Ctrl+Z. This will 
    playback the video in full-screen mode. In order to go back to the
    window mode, press Space in full-screen mode and it will resume 
    playback in the restored MPEG window.   



VI - HINTS TO RESOLVE PROBLEMS AND BETTER PLAYBACK 
     =============================================

1.  The drivers are installed and the NS 2000 appears in the 
    "Device Manager" but the CD's won't play.

    Run SETUP from the second diskette (Applications) to create the 
    "REALmagic NetStream 2000" group. This group contains the 
    DVD-Station, README file, REALmagic Configuration, and Uninstall.

2.  The REALmagic Configuration can be run but when the DVD-Station is
    started (or the Media Player with an MPEG file ) the system hangs.

    Check the Device Manager for a conflict in the IRQ resources and 
    make the necessary change(s).

3.  After installing the first disk for the drivers, and run SETUP from
    the second disk, the following message comes up : "Driver cannot be
    loaded, another instance from the driver may be running".  Or when
    playing an MPEG file after the software installation, there is an
    error message  "MMSYSTEM 266 : undetectable error ...".

    Reseat NS 2000 in different PCI slots because of some of 
    the motherboards BIOSes handling of the resources.


4.  The MPEG files play and the audio can be heard but the video is a 
    solid color.

    Run "REALmagic Configuration" and select "Auto Calibration." Or, 
    make sure that the output of the Display Adapter is routed to the
    NS 2000 input and the Display Adapter's output is routed to
    the monitor.

5.  The picture is waving.

    Run "REALmagic Configuration," select "Border Adjust" and adjust 
    the STABILITY: smoothness of the two vertical sides.

6.  MPEG 1 files run normally, but DVD movies are shaky.

    Make certain that the DVD-ROM drive is connected as a Master on the
    IDE controller. Also you can turn ON the DMA flag in the 
    "Device Manager-DVD ROM drive-Settings-DMA."

7.  For DVD-ROMs that require high data transfer rates, it is better to
    have the DVD-ROM drive connected to an IDE controller with the 
    "Bus Master" mode activated.   
    
8.  Capturing of an MPEG frame from an encrypted DVD movie is not 
    supported because of Copyright issues. In other cases the capture
    feature gives its best results at a color depth of 64K (16 bits) 
    or higher.

9.  Playing VOB files using the Media Player might not show the best 
    performance because of different navigation schemes. Use the 
    DVD Station for this.

10. The playback of some DVD movies might jump unvoluntarily to different
    parts of the movie. Fix this by : Start - Run - MSCONFIG - General -
    Advanced - Disable UDF file system. This is under Win 98.
  	 
11. Video is fine on VGA but is Black and White on TV.
 
    Please see section for TV-Out.

12. When watching the movie on TV, the picture gets dimmer and brighter
    at short intervals and with some movies some yellow horizontal
    lines appear on the TV screen.

    The TV set is connected to the PC system via a VCR or an alike 
    device.  This device initiates the Macrovision protection of the
    movie.  Connect the TV directly to the PC system.

13. The S-Video connector on Hollywood Plus is a 7-hole jack and
    my S-Video cable has a 4-pin socket only.

    The 4-pin cable is compatible with the 7-pin socket.  There are
    more pins on the 7-pin socket to provide for the composite TV
    output.

14. I lost the S-Video/Composite Adapter cable and have no access to
    another one.

    Order another one from your supplier.  In the USA, you can check
    the phone number or the email address of the fulfillment center on
    the web site . The  pinout of this adapter is as follows :

          _________
	 /         \
	|  7  6  5  |
	| 4 3   2 1 |
	|           |
	 \  OOOOO  /
	  ---------

	1:GND
	2:Composite
	3:GND
	4:GND
	5:Luma
	6:not connected
	7:Chroma
            

15.  You want DVD Station to check your DVD-ROM first and it has a 
     drive letter after the CD-ROM.  

     DVD Station allows you to set your preferred drive (Options -
     Tab : Play List).

16.  You see the video but no audio.

     - Try first the speakers plugged in NS 2000 and be sure the
       output from DVD Station is Stereo.
     - Then check the audio jumper cable from the output of NS 2000
       to the input of the sound card. If no sound, check the
       volume mixer to have Line-in NOT muted or at low level.
     - If you are using a Dolby Digital Receiver, make sure that it 
       accepts AC-3 streams and your setting in DVD Station is AC-3.
    

17. The maximum refresh rates allowed with the NS 2000 MPEG
    playback depends on a combination of the display adapter, and
    the monitor and some of these combinations may show
    a little degradation in the desktop display because of the 
    overlay. The MPEG playback is not affected.  However, the 
    following can be used as a guideline:

		 640 x  480	100 Hz
		 800 x  600	100 Hz
		1024 x  768	 85 Hz
		1152 x  864	 75 Hz
		1280 x 1024	 60 Hz 
		1600 x 1200	 60 Hz

18. The NS 2000 does NOT support the MP3 files playback.

19. You have a third generation DVD-ROM drive (RPC2 specs that require
    a region code on the drive) and you cannot playback movies.

    Run the manufacturer utility for this drive to set the region code
    to your country code.

20. You can add the option "/f=filename" on the command line of
    DVD Station to allow the direct playback of the file.


21. What is the pinout of the VGA signals on the pass-thru cable ?

       View of the 9 pin socket of the pass-through cable,
       seen from the bracket:
                         
                         _________
                        /_________\
                       |           |
                       | 9    8  7 |
                       |  6 5 4 3  |
                        \   2 1   /
                         ---------

                       1:Blue  IN
                       2:GND
                       3:Green IN
                       4:GND
                       5:Vsync IN
                       6:Hsync IN
                       7:Red   IN
                       8:SDA (from pin12 of DB15) - for PnP monitors
                       9:SCL (from pin15 of DB15) - for PnP monitors

 ======================================================================

	END   OF    FILE

