Corrective Service Facility disks for installing OS/2 FixPaks, release F.127

This ZIP file is a replacement for the previous WKICKR.ZIP file. It contains
updated CSF disk images called CSFBOOT.1DK and CSFBOOT.2DK. These are to be
used in place of WARPBDSK.1DK and WARPBDSK.2DK that were contained in the
original WKICKR.ZIP file.

To create diskettes from the disk image files you need LOADDSKF.EXE which is
included in this ZIP file.

Note: LOADDSKF.EXE is also on any CD-ROM version of OS/2.

Place a blank, formatted 1.44MB diskette in A: (or B:, whichever is your
3.5inch floppy drive).

Enter LOADDSKF CSFBOOT.1DK A: to create the 1st diskette

Place anopther blank, formatted 1.44MB diskette the same drive.

Enter LOADDSKF CSFBOOT.2DK A: to create the 2nd diskette

Save these diskettes for use when installing any OS/2 3.0 (Warp) or any OS/2
2.11 Fixpak starting with XR_A096 or later.

The disk image files should have the following file attributes

12-01-95  11:22a   1051706  csfboot.1dk
12-01-95  11:22a    961811  csfboot.2dk

*=============================================================================(

APAR reported problems fixed in initial release
-------------------------------------------

APAR= PJ17143
 IN THE CSF 2B 3 DISKETTE VERSION OF THE WKICKER DIKETTES THERE
 IS AN ICCORECT PROMPT ON THE FIRST DISK AFTER BOOT

APAR= PJ17191
 WHEN FIXPAK IS UPDATING DEFAULT DIRECTORIES, THE TITLE OF THE
 WINDOW IS INCORRECT

APAR= PJ17193
 IP07060 'KICKER' DISKS DISPLAY INCORRECT INFORMATION

APAR= PJ17195
 FIXTOOL 2-B ERRORS IN HELP TEXT


Additional problems fixed in release F.127
-------------------------------------------

APAR=PJ17911

 NO RESPONSE IS OBSERVED WHEN SERVICE BUTTON ON FRENCH OR OTHER
 NLV FIXPAK TYPE B BOOT DISKETTE IS PRESSED.

APAR=PJ17201

 SYSTEM HOSED AFTER INSTALLING FIXPAK XR_S091 (WITH FIXTOOL 2-B)

APAR=PJ17469

 BACKOUT A FIXPACK (FIXPAK 91), FSERVICE HANGS AFTER BACKING
 OUT COMPLETE.

APAR=PJ18262

 FIXPAK FSERVICE IS NOT SETTING THE ARCHIVE BIT ON FILES THAT IT
 UPDATES

APAR=PJ17973

 ERROR MSG CSF0222E WHEN TRYING TO COMMIT XRW005

APAR=PJ17919

 FSERVICE ACCESSES DRIVES OTHER THAN TARGET DRIVE SPECIFIED IN
 THE RESPONSE FILE DURING FIXPAK INSTALLATIONS.

APAR=PJ19008

 FSERVICE DOESNOT CLEANUP .DMD FILES FROM THE ROOT DIRECTORY
 AFTER SEMAINT IS RUN

APAR=PJ18369

 ERROR ON " CSF0294: ARCHIVING IS DISABLED FOR THE PRODUCT ... "
 WHEN APPLYING FIXPAK XRW005

APAR=PJ18491

 FIXPAK BACKOUT TRIES TO BACKOUT FILES THAT ARE NOT PRESENT AND
 WILL FAIL WITH ERROR UNPACKING THE FILE CSF0296.

APAR=PJ17975

 WHEN THE CONFIG.SYS HAS LINES > 512 CHARACTERS, SERVICE.EXE
 GIVE A SYS3175 ERROR MESSAGE.

APAR=PJ17930

 FIXPAK INSTALL DOES NOT UPDATE WINOS2 FILES IN THE WINOS2
 DIRECTORY AND SUBDIRECTORIES.

APAR=PJ19737

 FSERVICE LOG IS DISPLAYED ON THE SCREEN IF REPSONSE FILE DOES
 NOT HAVE :LOGFILE AND /L1: ON COMMAND LINE IS MISSING OR INVALID

APAR=PJ19601

 SYS3175 ON FSERVICE.EXE FIXPAK XR_W009 ON WARP (562260100)

APAR=PJ19821

 REDIRECTED INSTALLATION OF FIXPAK FAILS WITH CSF0212 AND CSF0248
 ERRORS DEPENDING ON THE DATE OF FSERVICE.EXE BEING USED.

APAR=PJ19790

 FSERVICE FAILS TO UPDATE THE OS2KRNL FILE IF USED IN PM MODE

APAR=PJ20467

 IBMCFLK DEVICE STATEMENT INSTALLED ABOVE 1ST IFS STATEMENT IN
 THE CONFIG.SYS.   CAUSING PROBLEM ON HPFS386 SYSTEMS.

APAR=PJ20469

 FIXPAK INSTALLATION ENDING WITH MESSAGE SAYING "NO PRODUCT TO
 UPDATE", WHILE THERE ARE PRODUCTS TO UPDATE ON THE SYSTEM.

APAR=PJ20470

 WARP FIXPAK (FIXTOOL-2B) INSTALLATION DOES NOT ALWAYS UPDATE THE
 WINOS2 FILES ON THE SYSTEM.

APAR=PJ20471

 004
 ON A SYSTEM THAT HAS BOTH OS/2 V2.11 AND WARP INSTALLED.

APAR=PJ20476

 FIXTOOL-2B: DURING FIXPAK INSTALLATION ON LOCKED FILES PANEL THE
 CLOSE  OPTION DOES NOT FUNCTION.

APAR=PJ20477

 FIXTOOL-2B: FIXPAK INSTALLATION PROCESS NOT CHECKING FOR CR/LF
 WHILE APPENDING THE CONFIG.SYS.

APAR=PJ20478

 FIXTOOL-2B: DURING FIXPAK INSTALLATION PROCESS USING FSERVICE
 PROGRESS INDICATOR DOESN'T SHOW LOCKED FILES.

APAR=

 DEFECT 139103: FixPak shows no progress on progress bar
