Windows 98 setup information file (acer98.inf)for Acer monitors.  
 
This Acer monitors Windows98 Setup Information file (acer98.inf) is the most updated  
version of the AcerView color monitor .inf file for Windows 98. After the file  
is installed, the system, due to its Plug & Play feature, will automatically  
read the file and detect the resolution settings of both the VGA card and your  
monitor. If the maximum VGA card resolution is selected and is higher than that 
of the AcerView Monitor, the system will automatically adjust the resolution to  
the maximum capacity of the monitor. 
 
Since Acer Peripherals, Inc. constantly introduces new monitors, we strongly  
recommend you to update the acer98.inf file to optimize the performance of your  
monitor. 
 
How to update the Windows 98 setup information for all Acer monitors  
 
Please follow steps below to update the acer98.inf file for Windows98.  
 
(1) Unzip the enclosed Acer98.zip file
    unzip the Acer98.inf into your windows\system directory; unzip the *.icm files into your windows\system\color directory.  
(2) Activate Windows 98. 
(3) Click Start and select "Settings/Control panel". 
(4) Click icon "Display". 
(5) Select "Setting". 
(6) Click the button "Change Display Type" or "Advanced Properties". 
(7) Click the button "Change" in monitor type item. 
(8) Click the button -- "Have disk". 
(9) Input path of the acer98.inf file, and click OK button. 
(10) Windows 98 will select a correct name automatically for your monitor. 
Click OK when the process ( ICM profile installed ) is finished.  