
Circuit Shop IC Library
=======================

L7400.CS1 - ICs in range 7400 - 7449
=========
   7400 - Quad 2-input NAND gates
   7401 - Quad 2-input open-collector NAND gates
   7402 - Quad 2-input NOR gates
   7403 - Quad 2-input open-collector NAND gates
   7404 - Hex inverters
   7405 - Hex open-collector inverters
   7406 - Hex open-collector high-voltage inverters
   7407 - Hex open-collector high-voltage buffers
   7408 - Quad 2-input AND gates
   7409 - Quad 2-input open-collector AND gates
   7410 - Triple 3-input NAND gates
   7411 - Triple 3-input AND gates
   7412 - Triple 3-input open-collector NAND gates
   7413 - Dual 4-input NAND gates with schmidt-trigger inputs
   7414 - Hex inverters with schmidt-trigger inputs
   7415 - Triple 3-input open-collector AND gates
   7416 - Hex open-collector high-voltage inverters
   7417 - Hex open-collector high-voltage buffers
   7418 - Dual 4-input NAND gates with schmidt-trigger inputs
   7419 - Hex inverters with schmidt-trigger line-receiver inputs
   7420 - Dual 4-input NAND gates
   7421 - Dual 4-input AND gates
   7422 - Dual 4-input open-collector NAND gates
   7424 - Quad 2-input NAND gates with schmidt-trigger line-receiver inputs
   7425 - Dual 4-input NOR gates with enable input
   7426 - Quad 2-input open-collector high-voltage NAND gates
   7427 - Triple 3-input NOR gates
   7428 - Quad 2-input NOR gates with buffered outputs
   7430 - 8-input NAND gate
   7432 - Quad 2-input OR gates
   7433 - Quad 2-input open-collector NOR gates
   7434 - Hex non-inverters
   7437 - Quad 2-input NAND gates with buffered outputs
   7438 - Quad 2-input open-collector NAND gates with buffered outputs
   7440 - Dual 4-input NAND gates with buffered outputs
   7442 - BCD to decimal decoder
   7445 - BCD to decimal decoder
   7447 - BCD to 7-segment decoder with ripple blank input (active low outputs)
   7448 - BCD to 7-segment decoder with ripple blank input (active high outputs)
   7449 - BCD to 7-segment decoder

L7450.CS1 - ICs in range 7450 - 7499
=========
   7451 - 2-wide 2-input and 2-wide 3-input AND-NOR gates
   7454 - 4-wide 2/3-input AND-NOR gate
   7455 - 2-wide 4-input AND-NOR gate
   7458 - 2-wide 2-input and 2-wide 3-input AND-OR gates
   7474 - Dual D-type positive edge-triggered flip-flops
   7476 - Dual JK negative edge-triggered flip-flops
   7483 - 4-bit binary full adder with fast carry
   7485 - 4-bit magnitude comparator with cascade inputs
   7486 - Quad 2-input EXCLUSIVE OR gates
   7490 - 4-bit asynchronous decade counter with /2 and /5 sections, set and reset
   7492 - 4-bit asynchronous divide-by-12 counter with /2 and /6 sections and reset
   7493 - 4-bit asynchronous binary counter with /2 and /8 sections and reset

===
EOF
===
